**Kapazitiver Bodenfeuchtigkeitssensor V2.0 Datenblatt**

**Features**

* Supports Gravity 3-Pin interface
* Analog output

**Applications**

* Garden plants
* Moisture detection
* Intelligent agriculture

**Specification**

* Operating Voltage: 3.3 ~ 5.5 VDC
* Output Voltage: 0 ~ 3.0VDC
* Interface: PH2.0-3P
* Dimension: 98mm \* 23mm (3.86in x 0.905in)
* Weight: 15

